"The landing light circuit breaker switch failed," says a mechanic. "This switch was replaced by AD2008-13-17 IAW SB24-3807. It is the third or fourth switch to fail since being installed in our fleet of Bonanza and Baron aircraft, a total of nine *(planes)*. This AD has caused a higher failure rate of our circuit breaker switches since compliance with this AD. *(I believe)* this new switch called for in the AD is inferior to the switch it has replaced." *(Switch P/N: 35-380132-103. The SDRS database reflects this switch 74 times—see also the next Alerts article. It would have been helpful had you indicated an estimated average time experienced from the old switch—Ed.)*

Part Total Time: 2,497.9 hours